Maxon:

<https://www.maxongroup.com/maxon/view/product/motor/ecmotor/ecflat/ecflat60/614949>

| Nominal voltage | 24 V |
| --- | --- |
| No load speed | 4300 rpm |
| No load current | 497 mA |
| Nominal speed | 3240 rpm |
| Nominal torque (max. continuous torque) | 536 mNm |
| Nominal current (max. continuous current) | 9.28 A |
| Stall torque | 4300 mNm |
| Stall current | 81.9 A |
| Max. efficiency | 85 % |

<https://www.maxongroup.com/maxon/view/category/motor?etcc_cu=onsite&etcc_med_onsite=Product&etcc_cmp_onsite=ECX+SPEED+program&etcc_plc=Overview-Page-Brushless-DC-Motors&etcc_var=%5bcom%5d%23en%23_d_&target=filter&filterCategory=ECX>

| Nominal voltage | 18 V |
| --- | --- |
| No load speed | 4450 rpm |
| No load current | 829 mA |
| Nominal speed | 3470 rpm |
| Nominal torque (max. continuous torque) | 896 mNm |
| Nominal current (max. continuous current) | 20.8 A |
| Stall torque | 10300 mNm |
| Stall current | 269 A |
| Max. efficiency | 89 % |